Heat gains per defined room or zone can be generated. The required timestep and numbering of rooms/zones is defined from the 'Gains/Espr Input Definition' tab on the right of the GUI. (Note: room/zone names are only required for ESPr gains file generation). 

The output for each room/zone contains five columns of data. These comprise: occupant gains (convective, radiant and latent), and combined lighting, appliance and hot water gains (convective and radiant). All data is in Watts. 